Auto\_PO\_Export *User Guide*

This user guide corresponds to the ***Auto\_PO\_Export***, this is a useful tool to export automatically ***Assembly groups*** **[AG]** documentation from the Ulysses software.

# Inhalt

[1. Configuring the export 1](#_Toc24978849)

[1.1. 1](#_Toc24978850)


# Configuring the export


There are two steps for the tool configuration, the first is a **“Record”** phase, where you can set the referring **[AG]** name and record the mouse and key events in order to create an export of the **[AG]** documentation, as result of this phase you will save an instruction file named ***instructions.json*** containing the recorded events.

The second phase is the **“Playing”** phase; here you just have to run the **“player.exe”** program. It will read the saved instructions from the **“Record”** phase (***instructions.json***) and replicate it in order to export the same **[AG]** documentation.

## Record Phase

### Open the *recorder.exe*, set the [AG] and *Ulysses PID.*

Please register to Ulysses first and then go to the ***recorder*** folder and run the ***redorder.exe.*** The see the following window will appear***.***

* Set the **[AG]** number on the field ***“Assembly Group”, press “Return” to apply.***
* Set the ***Ulysses PID*** on the field ***“Ulysses PID” , press “Return” to apply.*** You can read the Ulysses PID from the tasks manager, consider the following image:

### Recording Rules

For the recording of actions are some rules to follow, please consider that only the following events will be cached:

* Right Click
* Left Click
* “Return” Key pressed
* “Delete” Key pressed
* “Space” Key pressed

Right and Left clicks will be saved and reproduced on the same position they was made.

The first time the “***Return***” Key is pressed should be made on the ***Artikelnummer*** field from the Ulysses search window; this will tell the program to write there the **[AG]** number you give on the ***recorder.***





Figure 1: The first time the Return key is clicked means for the program, to write there and search the given Assembly group number.

The second time the Return Key is pressed will tell the program to write there the ***table name,*** of the **[AG]** number exported from Ulysses, in order to save it on the right path. The program will create a new folder called “***Projects***” on the top directory of the ***Auto\_PO\_Export*** Tool, and save the exported data there.




Figure 2: Top directory of the Auto\_PO\_Export. The "Projects" folder will contain the exported data.

### Click on the “Record” button.

The ***Recording*** will start, on the left upper corner of your screen will appear the stop Button, please click it, to stop the recording actions (It might appear a console window showing the clicked positions).




Figure 3: Recording state, just the stop button will be available.